Calibration (FLUKE Mulitmeter)

Measurements:

Standby: 0.0247A

Full load: 1.012A